DEXIS 950+ Manual Installation process

1. Install DEXIS 9 on the server using the CD file using DEXmenu, or the daDEXus.exe in the Engl-US folder.
   1. Follow the prompts and if asked for the data folder, this will be the local folder. Ex: E:\dexis\data  
      The rest of the prompts can remain default.
2. After it is installed, go to the data\download folder and rename DEXlib-Platinum.exe and the KaVo\_IO-Sensor\_Driver.exe.
   1. You can just add a ‘1’ or the DEXIS version number to the end of the name.
3. Run each program manually on each machine in the order: Defaults can be used for each
   1. da9XXus.exe
      1. If an error occurs stating a path cannot be accessed, manually change the data-path for the currently installed instance.
         1. C:\dexis\dexis.ini – Modify ‘xdata=’ field to be the UNC path to the database: ex. [\\server\dexis\data](file:///\\server\dexis\data)  
            so the line should read: “xdata=\\server\dexis\data”
         2. This should resolve the drive accessibility issue and the install should continue.
   2. DEXlib-Platinum1.exe
   3. KaVo\_IO-Sensor\_Driver1.exe
      1. If an existing driver is installed, extra prompts may appear asking to close open programs, It is ok to click through this and allow the program to close.
4. After installation, restart the machine.
5. KaVo Connect registration will appear. Register 1 machine going through First Time Practice Registration.
   1. This will make a file on the server which will update the rest of the machines.
   2. The other machines may need to be restarted to update the Registration code.